The Weather.csv and Radiation.csv are from Baltimore, MD, Baltimore-Washington Intl AP
USAF	WBAN	YEAR
724060 	93721 	2018


The LCScale_11x11Grid is archived for land cover scaling analysis, 
Input 11 x 11 array map inputs of imperviouscover.txt and treecover.txt span the range of 0 to 100% with 122 unique cases.  
Outut processed with z_b_3DMap_CoolAir_Temperatures.py selecting 11x11 and D for daily; 12x12 output arrays can be processsed with same code. 

Typically, tree cover and impervious cover increment from from 0, 10, 20, .., 90, 100%. 

Use a BlockGroupMap.txt file that contains 122 distinct values to obtain temperature outputs across these 122 cases. 
Use the <PrintBlockGroupRange>1,122</PrintBlockGroupRange> to generate BlockGroup1.txt or BlockGroupDaily1.txt.

A successful run typically requires at least 5 days of output. 
After launching the script in the Xterm window, there will be a prompt for array size (11 or 12) and inputs options (daily or hourly).
You can rotate the plot while viewing. 
Once the script is complete, graphic files are stored in the output subfolder, called Daily_Metrics (or Hourly_Metrics). 
This stored version of the test case has been run for the full 122 cases in order to save performance details.  